	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-MZ14KLW
용 도	영사용 기기	밝 기	14,000안시
A. 제품 이미지 LCD Projector

	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-MZ14KLW
용 도	영사용 기기	밝 기	14,000안시
B. 특 징 (Features) ** 14,000안시 WUXGA의 해상도, 3LCD Laser 광원 프로젝터 ** * 3LCD 레이저 광원 프로젝터 - 3LCD 레이저 광원 프로젝터 - 14,000 ANSI Lumen 밝기 - WUXGA 해상도 1,920 x 1,200 의 16:10 화면비율 - 3,000,000 : 1의 고명암비 * 선명한 화질 - Dynamic Contrast NX 기능을 통한 고명암 실현 - Pure White Generator 로 고휘도와 풍부한 색채 실현 * 더 쉬워진 유지보수 - 정상 모드 시 20,000시간의 레이저 광원 수명 - 액체 냉각 시스템 및 방진 구조로 장기적인 안정성 - 설정 변경 및 상태 확인을 위한 정보 모니터 * 뛰어난 시스템 유연성 - 상하좌우, 360도 다양한 각도 설치 - 빠른 시작 및 퀵오프 - 원활한 설치를 위한 스마트 프로젝터 컨트롤 앱 - 기하학적 조정으로 사다리꼴 왜곡 및 커프 스크린 수정 - 프리그리드를 통해 국소 왜곡의 핀포인트 보정 기능 - Geometry Manager Pro 소프트웨어를 탑재하여 내장기능 확장을 통해 PC에서 조정 가능 - 커브된 화면에서도 유연한 블랙레벨 보정이 가능 * 최상의 기능 탑재 - 페일오버 기능으로 소자 중 하나가 오작동할 경우 지속적 투영 가능 - 백업 입력 기능을 통한 신뢰성 향상 - 데이터 클로닝 기능이 USB 메모리와 호환 - 이미지 리모트 확인을 위한 리모트 프리뷰 - 4K 신호 입력 지원 - 의학용 이미징 표준 규격에 충족된 DICOM 시뮬레이션 모드로 X-ray 이미지 디스플레이 구현

규  격  시  방  서

품  명

비디오 프로젝터

모 델

PT-MZ14KLW

용  도

영사용 기기

밝 기

14,000안시

C. 규  격(Specifications)

Item	Description
패널	25.4 mm (1.0”) (16:10 비율) LCD × 3
해상도	WUXGA (1,920 x 1,200 pixels)
광 원	Laser diodes (광원수명 : 20,000H)
밝 기	14,000 Lumens
명암비	3,000,000:1 (Full On/Full Off)
주변조도비	85%
스크린 사이즈	2.03–15.24 m (80–500 in), 16:10 aspect ratio
	2.54–10.16 m (100–400 in), 16:10 aspect ratio(with ET-EMU100)
	2.03–12.7 m (80–500 in), 16:10 aspect ratio(with ET-EMT800)
렌즈	Optional powered zoom lenses
터미널	HDMI IN	HDMI 19-pin x 1 (Compatible with HDCP 2.3, DeepColor, 4K/60p signal input,CEC supported)
	SDI IN	BNC x 1 (3G/HD/SD-SDI input)
	SERIAL/MULTI PROJECTOR SYNC IN	D-sub 9-pin (female) x 1 for external control (RS-232C compliant)
	SERIAL/MULTI PROJECTOR SYNC OUT	D-sub 9-pin (male) x 1 for link control (RS-232C compliant)
	REMOTE 1 IN	D-sub 9-pin (female) × 1 for external control (parallel)
	REMOTE 2 IN	M3 x 1 for wired remote control
	REMOTE 2 OUT	M3 x 1 for link control (for wired remote control)
	DIGITAL LINK	RJ-45x1fornetworkandDIGITALLINKconnections(HDBaseTTMcompliant), PJLink(class2)compatible,100Base-TX,Art-Netcompatible, HDCP2.3compatible,DeepColorcompatible,4K/60psignalinput
	LAN	RJ-45 x 1 for network connection, 10Base-T, 100Base-TX (Compatible with PJLink™ [Class 2], Art-Net)
	DC OUT	USB Connector (Type A) x 1 (for power supply (DC 5V, maximum 2A))
	USB	USB Connector (Type A) x 1 (Output 5 V/2 A)
키스톤보정	수직:±45°(±5°withET-EMU100,±14°withET-EMW200/EMW300,±22°withET-EMW400/EMW500) 수평:±40°(±8°withET-EMW200/EMW300,±15°withET-EMW400/EMW500)
렌즈쉬프트	수직:±60%(-20~+50%withET-EMU100,±40%withET-EMW200,±50%withET-EMW300)(powered) 수평:±20%(±19%withET-EMW200)(powered)
소음	Nomal : 35 dB / Quiet : 30 dB
전원	100-240 V AC, 50/60 Hz
소비전력	615W (Nomal : 520 W / Quiet : 340 W / Shutter : 10 W)
크기 (W×H×D)	650 x 211 x 440 mm (Without lens)
무게	Approximately23kg