	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-REZ80
용 도	영사용 기기	밝 기	8,000안시
A. 제품 이미지 1-Chip DLP Projector

	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-REZ80
용 도	영사용 기기	밝 기	8,000안시
B. 특 징 (Features) ** 진화된 1chip DLP 프로젝터 ** * 8,000lm 1chip DLP WUXGA 프로젝터 - 1-Chip 프로젝션 시스템 - 8,000 ANSI Lumen 밝기 - WUXGA 해상도 1,920 x 1,200 의 16 : 10 화면비율 - 명암비 25,000 : 1 * 매끄러운 투사로 몰입도 향상 - 향상된 Dynamic Contrast를 통해 고대비 비주얼 투사 - Rich Color Enhancer를 통해 적절한 작동모드를 선택하여 최적화 - Gradation Smoother을 이용해 음영처리된 색상 그라데이션에서 밴딩 감소 - Detail Clarity Processor 4로 선명도를 향상 - 블랙레벨을 유연하게 조정하여 왜곡없이 화면에 대칭적으로 적용(블렌딩) - 와이드 스크린 입력신호 지원 * 유연성과 확장성을 통해 시간을 절약해주는 워크플로우 - 완전히 새로운 렌즈 라인업과 함께 적용 - 인텔SDM 지원슬롯을 통한 폭 넓은 확장성 - 사용자 정의 테스트 패턴을 가져오기 및 저장 기능 - NFC 기능으로 설정 전 준비시간 절양 - 원격 제어를 통한 유연한 화면 조정 - Geo Pro용 사전 활성화된 업그레이드 키트 소프트웨어 - 프로젝터 본체 피치와 각도의 변화를 감시하여 OSD메뉴에 표시하는 자이로센서 탑재 * 새로운 컴팩트 본체로 유지관리가 필요없는 프로젝션 지원 - 방진 광학 엔진 및 액체 냉각 시스템 - 모니터링을 위한 원격 미리보기 LITE - 백업 입력 이중화 - 멀티 레이저 구동 엔진 * 다양한 추가 기능 - 멀티스크린 지원 시스템 - DICOM 시뮬레이션 모드 - 다중 장치 밝기 및 색상 제어

규  격  시  방  서

품  명

비디오 프로젝터

모 델

PT-REZ80

용  도

영사용 기기

밝 기

8,000안시

C. 규  격(Specifications)

Item	Description
패널	0.8” (16:10 비율) 1chip DLP
해상도	WUXGA (1,920 x 1,200 pixels)(with Quad Pixel Drive)
광 원	Laser diode (광원수명 - Nomal : 20,000h / Eco : 24,000h)
밝 기	8,000 Lumens
명암비	25,000:1
주변조도비	90%
스크린 사이즈	70-700 in, 16:10 aspect ratio
렌즈	Power zoom (throw ratio 1.36–2.10:1), Power Focus (F1.84-2.31) (optional lenses also available)
단자	HDMI 1IN/ 2IN	HDMI x 2 (Deep Color, compatible with HDCP 2.3, 4K/60p signal input4)
	DisplayPort	DisplayPort x 1 (Deep Color, compatible with HDCP 2.3, 4K/60p signal input4)
	MULTI SYNC IN	BNC x 1 (TTL high impedance)
	MULTI SYNC OUT	BNC x 1 (TTL output: Maximum 10 mA)
	SERIAL IN	D-sub 9-pin (female) x 1 for external control (RS-232C compliant)
	SERIAL OUT	D-sub 9-pin (male) x 1 for link control (RS-232C compliant)
	REMOTE 1 IN	M3 stereo mini-jack x 1 for wired remote control
	REMOTE 1 OUT	M3 stereo mini-jack x 1 for link control (for wired remote control)
	REMOTE 2 IN	D-sub 9-pin (female) x 1 for external control (parallel)
	LAN	RJ-45 x 1 for network connection, PJLink™ (Class 2) compatible, 10Base-T/100Base-TX, Art-Net compatible
	USB	USB connector (Type A) x 1 for optional AJ-WM50 Series Wireless Module/USB memory stick
	DC OUT	USB connector (Type A) x 1 (for power supply, DC 5 V, 2 A)
	SLOT	Open slot for function boards, Intel® SDM compatible
렌즈쉬프트	수직: ±60 % (powered) , 수평: ±29 % (powered)
키스톤	수직: ±40° (powered) , 수평: ±40° (powered)
소음	Nomal/Eco : 35 dB / Quiet : 32 dB
전원	100-240 V AC, 50/60 Hz
소비전력	Nomal 640W / Max : 700W / Eco : 425W / Standby : 12W
크기 (W×H×D)	498 x 212 x 648 mm (including standard zoom lens)
무게	Approximately 28.7kg (including standard zoom lens)