	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-REQ80
용 도	영사용 기기	밝 기	8,000안시
A. 제품 이미지 1-Chip DLP Projector

	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-REQ80
용 도	영사용 기기	밝 기	8,000안시
B. 특 징 (Features) ** 차세대 1-Chip 4K 프로젝터 ** * 차세대 1-Chip 4K 프로젝터 - 1-Chip 프로젝션 시스템 - 8,000 ANSI Lumen 밝기 - 4K 해상도 3,840 x 2,400 의 16 : 10 화면비율 - 명암비 25,000 : 1 * 새로운 차원은 드라마틱한 비주얼 프로덕션 - 쿼드픽셀드라이브를 통해 부드러운 4K 이미지 생성 - 색상 최적화기술을 통한 선명하고 정확한 표현 - 그라데이션 스무더를 통해 색상 그라데이션의 밴딩 최소화 - 향상된 Dynamic Contrast를 통한 명암 대비 - 곡선 스크린의 블랙 레벨 조정 - 기하학적 보정 적용 이후 나타날 수 있는 블랙 레벨 조정 - 와이드 스크린 입력 신호 지원(21:9 신호 지원) * 간편한 워크플로우, 향상된 확장성 - 새로운 렌즈 라인업 - Intel SDM 지원 슬롯 - 사용자 지정된 테스트 패턴 저장 및 가져오기 기능 - QR코드 스캔을 통해 최대 64개 프로젝터 동시 제어 및 설정 조절 가능 - NFC 기능 - 프로젝터의 각도변화를 감지하여 그래픽으로 표시 * 새로운 캐비닛 설계 - 방진광학엔진 및 액냉 시스템 - LITE를 사용하여 투사하기 전 모니터링 가능 - 백업 입력 이중화 - 멀티 레이저 드라이브 엔진 *기타 - DICOM 시뮬레이션 모드 - 멀티스트린 지원 시스템 - 빠른 시작 및 빠른 종료

규  격  시  방  서

품  명

비디오 프로젝터

모 델

PT-REQ80

용  도

영사용 기기

밝 기

8,000안시

C. 규  격(Specifications)

Item	Description
패널	0.8” (16:10 비율) 1chip DLP
해상도	4K (3,840 x 2,400 pixels)(with Quad Pixel Drive)
광 원	Laser diode (광원수명 - Nomal : 20,000h / Eco : 24,000h)
밝 기	8,000 Lumens / 8,200 lumens (Center)
명암비	25,000:1
주변조도비	90%
스크린 사이즈	70-700 in, 16:10 aspect ratio
렌즈	Power zoom (throw ratio 1.36–2.10 :1), Power Focus (F = 1.84-2.31 mm)
단자	HDMI 1IN /HDMI 2IN	HDMI x 2 (Deep Color, compatible with HDCP2.3, 4K/60p signal6)
	DisplayPort IN	DisplayPort x 1 (Deep Color, compatible with HDCP 2.3, 4K/60p signal6)
	MULTI SYNC IN	BNC x 1 (TTL high impedance)
	MULTI SYNC OUT	BNC x 1 (TTL output: Maximum 10 mA)
	SERIAL IN	D-sub 9-pin (female) x 1 (for external control (RS-232C compliant))
	SERIAL OUT	D-sub 9-pin (male) x 1 (for link control (RS-232C compliant))
	REMOTE 1 IN	M3 stereo mini-jack x 1 (for wired remote control)
	REMOTE 1 OUT	M3 stereo mini-jack x 1 (for link control (for wired remote control))
	REMOTE 2 IN	D-sub 9-pin (female) x 1 (for external control (parallel))
	LAN	RJ-45x1(fornetworkconnection,PJLinkTM(class2)compatible,10Base-T/100Base-TX, Art-Netcompatible)
	USB	USB connector (Type A) x 1 (for optional AJ-WM50 Series Wireless Module/USB memory stick)
	DC OUT	USB connector (Type A) x 1 (for power supply, DC 5 V, total of 2 A)
	SLOT	SLOT x 1 (for function boards, Intel® SDM compatible)
렌즈쉬프트	수직: ±60 % (powered) , 수평: ±29 % (powered)
소음	Nomal/Eco : 35 dB / Quiet : 32 dB
전원	100-240 V AC, 50/60 Hz
소비전력	Nomal : 575W / Max : 730W / Eco : 455W / Standby : 12W
크기 (W×H×D)	498x212x538mm
무게	Approximately 27kg

\