	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-CMZ50
용 도	영사용 기기	밝 기	5,200안시
A. 제품 이미지 Ultra-Short Throw LCD Projector

	규 격 시 방 서
품 명	비디오 프로젝터	모 델	PT-CMZ50
용 도	영사용 기기	밝 기	5,200안시
B. 특 징 (Features) ** 최소 음영을 통해 초단거리에서 대형 이미지를 전송하는 레이저 프로젝터 ** * 최소 음영을 통해 초단거리에서 대형 이미지를 전송하는 레이저 프로젝터 - 3LCD 프로젝션 시스템 - 5,200 ANSI Lumen 밝기 - WUXGA 해상도 1,920 x 1,200 의 16 : 10 화면비율 - 명암비 3,000,000 : 1 * 공간이 제한된 장소에서 대형 이미지 투영 - 약 1cm 거리에서 80인치 이미지를 전달 가능 - 렌즈가 발표자보다 앞에있어 음영과 눈부심 감소 - 간편한 와이드스크린 콘텐츠 제공(21:9, 27:9 신호 수신) - Dynamic Contrast 모드 - Detail Clarity Processor 4 제공 * 설치,설정 및 조정 간소화 - 원격 제어를 통한 파워 센터 및 주변 초점 - Digital Zoom Extender 및 Digital Image Shift 기능 - 슬라이딩 및 기울기 조정이 가능한 월마운트 - Digital Link 연력릉 통한 4K 입력신호 수신 - USB 포트 포함 * 스트레스 없는 일상 업무 - 램프 프로젝터대비 31% 더 우수한 최대 전력 소비량 - 필터 재사용 가능 - 노트북 또는 스마트 폰에서 무선으로 프로젝트 수행 - PressIT 버튼을 통해 무선 프레젠테이션 시스템 가능 - 조기 경고 기능이 있는 다중 모니터링 및 제어 소프트웨어 옵션 * 추가 기능 - 내장 10W 스피커 - DICOM 시뮬레이션모드 - 360〫〫〫〫〫〫〫〫〫〬〬〬 설치

규  격  시  방  서

품  명

비디오 프로젝터

모 델

PT-CMZ50

용  도

영사용 기기

밝 기

5,200안시

Item	Description
패널	16.3mm (0.64”) (16:10 비율) LCD × 3
해상도	WUXGA (1,920 x 1,200), 2,304,000 pixels
광 원	Laser diodes (광원수명 - Nomal : 20,000h / Eco : 24,000h)
밝 기	5,200 Lumens
명암비	3,000,000:1 (Dynamic Mode/Dynamic Contrast 1/2)
주변조도비	85%
스크린 사이즈	2.03-3.05 m [80-120 in], 16:10 aspect ratio
렌즈	Fixed zoom, power focus, (throw ratio 0.235:1), F = 1.7, f = 2.81 mm
단자	HDMI 1 IN /2 IN	HDMI-19 pin x 2 (Compatible with HDCP 1.4, Deep color, 4K/30p signal input), CEC supported
	HDMI OUT	HDMI-19 pin x 1 (Compatible with HDCP 1.4, Deep color, 4K/30p signal output)
	COMPUTER IN	D-sub 15pin (female) x 1
	AUDIO IN	M3stereomini-jackx1
	VARIABLE AUDIO OUT	M3stereomini-jackx1
	SERIAL IN	D-sub 9-pin (female) x 1 for computer control (RS-232C compliant)
	LAN	RJ-45 x 1 for network control, 10Base-T, 100Base-TX, compatible with PJLinkTM (Class 2)
	DIGITAL LINK/LAN	RJ-45 x 1 for network and DIGITAL LINK connection, HDBase-T compliant, 100Base-TX, compatible with PJLinkTM (Class 2), HDCP, Deep Color, 4K/30p signal input
	USB(VIEWER /WIRELESS/DC OUT)	USB connector (Type A) x 1 for Memory Viewer function, optional AJ-WM50 Series Wireless Module , power supply (DC 5 V, maximum 2 A)
키스톤보정	수직 : ±3° / 수평 : ±3°
스피커	모노 10W
소음	Nomal/Eco : 35 dB / Quiet : 26 dB
전원	100-240 V AC, 50/60 Hz
소비전력	[MAX]325W(100–120V),310W(200–240V) [NORMAL]:290W(100–120V),280W(200–240V) [ECO]:215W(100–120V),205W(200–240V) [QUIET]:210W(100–120V),200W(200–240V)
크기(W×H×D)	495x160x421mm (not including lens or protruding parts)
무게	Approximately 9.5kg (with supplied lens)

C. 규  격(Specifications)